{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Výpočet","Fasády","Pomoc"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Výpočet","index":0,"n_rows":35,"n_cols":22,"rows_kept":35,"cut":false,"hidden":false,"merged":[[8,13,8,14]]}
["Výpočet tepelné zátěže podle ČSN 73 0548"]
[]
["Měsíc:",null,"M",4,null,"Teplota v místnosti",null,null,26]
["Orientace:",null,"Východ",90,null,"Ampl.kolísání teplot",null,null,7]
["Sklon:",null,null,90,null,"Celková prop. dif. radiace",null,null,0.85]
["Součinitel znečištění",null,null,{"$f":"IF($D$3=3,3,0)+IF($D$3=4,4,0)+IF($D$3=5,4,0)+IF($D$3=6,5,0)+IF($D$3=7,5,0)+IF($D$3=8,4,0)+IF($D$3=9,4,0)+IF($D$3=10,3,0)","v":4}]
["Korekce na čistotu atm.",null,null,"0,85"]
["Sluneční deklinace"]
["Hodina","Venkovní teplota","Sluneční azimut","Výška slunce","Úhel mezi normálou osluněného povrchu a směrem paprsků","Intenzita přímé sluneční radiace","Intenzita přímé sluneční radiace dopadající na stěnu","Intenzita difusní sluneční radiace","Intenzita celkové sluneční radiace","Celk. poměrná propustnost přímé sluneční radiace","Intenzita sluneční rad. procházející jednoduchým standartním zasklením","Intenzita difusní slun. rad. procházející jednoduchým standartním oknem","Rozdíl slun. azimutu a azimutu stěny","Délka stínu",null,"Osluněná plocha","Tepelné zisky konvekcí oknem","Tepelné zisky radiací oknem","Rovnocená sluneční teplota","Rovnocená sluneční teplota v době o y dřívější","Tepelné zisky konvekcí stěnou","Celkové zisky fasádou"]
[null,"te","a","h","Q","ID","IDS","Id","IC","TD","I0","I0dif","Ia-gI","e1","e2","Sos","QOK","QOR","tr","try","QSK","QSK"]
[null,"[°C]","[ °]","[ °]","[ °]","[W/m2]","[W/m2]","[W/m2]","[W/m2]","[-]","[W/m2]","[W/m2]","[ °]","[m]","[m]","[m2]","[W]","[W]","[°C]","[°C]","[W]","[W]"]
[1]
[2]
[3]
[4]
[5]
[6]
[7]
[8]
[9]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]

{"sheet":"Fasády","index":1,"n_rows":41,"n_cols":19,"rows_kept":41,"cut":false,"hidden":false,"merged":[]}
["číslo fasády","Orientace","azimut stěny","sklon","Plocha okna","Stínicí součinitel","Souč. prostupu tepla oknem","Tloušťka stěny","Plocha stěny","Souč. prostupu tepla stěnou",null,null,null,"Výsledky výpočtu"]
[{"$f":"+COUNT(A3:A12)","v":3},null,"g","a","Sok","s","Uok","d","Ss","Us",null,null,null,"březen",null,"W","v",null,"hod"]
[1,"východ",90,90,8,0.50400000000000011,1.4,0.3,10,0.3,null,null,null,"duben",null,"W","v",null,"hod"]
[2,"jih",180,90,8,0.50400000000000011,1.4,0.3,10,0.3,null,null,null,"květen",null,"W","v",null,"hod"]
[3,"západ",270,90,8,0.50400000000000011,1.4,0.3,10,0.3,null,null,null,"červen",null,"W","v",null,"hod"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"červenec",null,"W","v",null,"hod"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"srpen",null,"W","v",null,"hod"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"září",null,"W","v",null,"hod"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"říjen",null,"W","v",null,"hod"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"MAX",null,"W"]
[]
[]
["Hodina","Fasáda 1","Fasáda 2","Fasáda 3","Fasáda 4","Fasáda 5","Fasáda 6","Fasáda 7","Fasáda 8","Fasáda 9","Fasáda 10","CELKEM"]
["t","Qc1","Qc2","Qc3","Qc4","Qc5","Qc6","Qc7","Qc8","Qc9","Qc10","Qc"]
["h","[W]","[W]","[W]","[W]","[W]","[W]","[W]","[W]","[W]","[W]","[W]"]
[]
[1]
[2]
[3]
[4]
[5]
[6]
[7]
[8]
[9]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
["MAX"]

{"sheet":"Pomoc","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}